# Call Placement Menu

### RNA Retry Limit

Sets how many times the server tries to deliver a call placement message after a Ring No Answer call.

Enter: Number of retries, from 1 through 255

Default: 10 retries

### RNA Retry Interval

Sets how long the server waits between tries to deliver a call placement message after a Ring No Answer call.

Enter: Minutes, from 1 through 255

Default: 60 minutes

### Busy Retry Limit

Sets how many times the server tries to deliver a call placement message after a Busy call.

Enter: Number of retries, from 1 through 255

Default: 10 retries

### Busy Retry Interval

Sets how long the server waits between tries to deliver a call placement message after a Busy call.

Enter: Minutes, from 1 through 255

Default: 10 minutes

### Message Phone Length

Sets the maximum number of digits a user can enter for a call placement phone number.

Enter: Number of digits from 1 through 25

Default: 7 digits

### Recipient Count

Sets the total number of telephone numbers that the user can enter for a single message. This applies to the Call Placement optional feature.

Enter: Number of phone numbers from 0 through 190

Default: 190

### Maximum Message Length

Sets how long a message can be for a call placement phone number.

Enter: Minutes, from 0 through 60; 0 means no limit

Default: 5 minutes

Interactions & Limitations: The average length of call placement messages affects the number of ports in a pager line group.