# Assign Message Waiting Type to a Mailbox

## Web Console:

To assign message waiting indicators to a mailbox:

1. Edit the selected mailbox using the instructions under Edit Mailboxes.

2. On the Message Waiting tab, in the Message Waiting #1 field (or Message Waiting # 2 if #1 is used for another MWI application), assign the applicable Message waiting type from the table below:

Number | Message Waiting Type
--- | ---
0 | None
3 | DTMF to PBX
5 | Pager (See Pager Application)
7 | Program RS232
9 | Centrex RS232
11 | Centrex
16 | HIS PMS
17 | Unified Integration
21 | Hitachi PMS
28 | MiTAI Messaging

1. Click Save.

## Text Console

To assign message waiting indicators to a mailbox:

1. From the Main Menu, select (M) Mailbox Maintenance.

2. Select (C) Create New Mailboxes or (M) Modify Mailboxes and enter the number of the mailbox to which you want to assign a message waiting indicator.

3. Press Enter until Message waiting type #1: or, if #1 is used for another MW application, until Message Waiting Type #2: appears and then assign the applicable Message waiting type from the table above.

4. Press Enter to skip through each of the remaining mailbox configuration prompts. After the last prompt, the server displays the mailbox configuration, then prompts for the next mailbox number.

At this point, the parameter settings are saved and you can continue with mailbox configuration or exit.