# Mailbox Blocked Report (Blocked Billing Report)

## Overview

The Mailbox Blocked Report (sometimes called Blocked Billing Report) retains a special format and is usually sent out through the serial port to other databases. It presents the same information as the Billing Report but in blocked form—without titles or summaries.

Use this report when you want to organize the billing data into your own format, such as for an invoice or monthly statement.

## To Run the Mailbox Blocked Report

1. From the Main menu, select (R) Report Generation, (B) Billing, and then (M) Mailbox Blocked Report.

2. Complete steps 3 through 10 under Run the Billing Report.

## Reading the Mailbox Blocked Report (Field Descriptions)

To help you identify the field names and field lengths of statistics provided in the Mailbox Blocked Report, use the following table. All fields are right justified; all fields other than the mailbox number are blank-filled.

Field Name | Field Length (Number of Characters)
--- | ---
Mailbox number | 16
Department code | 10
User messages | 5
Caller messages | 5
Wakeup messages | 5
Logins | 5
Greets | 5
User connect time | 5
Caller connect time | 5
Disk usage | 10
Calls to pagers | 5
Calls for message delivery | 5
FCOS number (Repeated 16 times for line group billing.) | 3
LCOS number (Repeated 16 times for line group billing.) | 3
GCOS number (Repeated 16 times for line group billing.) | 5
Number of network messages | 5
Number of urgent network messages | 5
Number of network nodes sent to | 5
Number of network nodes sent urgent to | 5
Number of remote network recipients sent to | 5
Number of remote network recipients sent urgent to | 5
0.1-minute increments of network messages sent | 5
0.1-minute increments of network messages sent urgent | 5
0.1-minute increments of network nodes sent to | 5
0.1-minute increments of network nodes sent urgent to | 5
0.1-minute increments of remote network recipients sent to | 10
0.1-minute increments of remote network recipients sent urgent to | 10
Number of network receipt responses | 5
Number of network messages received | 5
Number of network urgent messages received | 5
0.1-minute increments of message length received over network | 5
0.1-minute increments of urgent message length received over network | 5