# Default Configuration Settings

The NuPoint Voice application is the only application that is pre-installed in the factory configuration. To add capabilities, and to meet the requirements of a particular site, you may need to change one or more of the defaults. You can use the Web Console or Text console to change the defaults.

The default configuration has the values shown in the following table.

Parameter | NuPoint Voice Default Setting
--- | ---
Administrator’s mailbox number | 998
Allow dial an extension for callers | N
Allow dial an extension for users | N
Allow multiple messages for outside caller | Y
Answer delay | 0
Attendant’s mailbox number | 999
Attendant transfer string | S+
Dial by name, last name first | Y
Exact match break | Y
General greeting mailbox number | None
Group name | None
Key 0 for attendant transfer | N
Line group number | 1
Line(s) in group | All on server
Mailbox dialing plan | 3,3,3,3,3,3,3,3,3
Number of names threshold | 3 names
Passcode length | 4 digits min. – 10 digits max.
Passcode trip count | 5
Passcode trip period | 24 hours
Pre-company name dial string | None
Pre-mailbox greeting dial string | None
Prompts language | English
Single digit access | None
Suppress mailbox number | None
System attendant’s extension | 0
Wait prompt | Y
Weekend days table | DDDDDNN
Work day | 8 a.m. – 5 p.m.

Parent topic: NuPoint Voice Application