# Trusted Networks

The page displays the default networks and an option to add a new network.

NOTE: The Trusted Networks page is not for managing trusted networks. To do so, use the Networks panel after initial configuration is completed.

## Selecting a Default Network

Select the check box from the list of default networks. Else, refer to the following section to add a new network.

## Adding a New Network

To add a new network to the list of trusted networks, do the following:

1. Select the check box against Add a new network option.

2. Enter the Network address.

3. Enter the subnet mask details in the Subnet mask or network prefix length field.

   NOTE: If this field is left blank, the system will assign a network prefix length of /24 for IPv4 networks.

4. Click Next after configuring the trusted network. The External Network Interface (WAN) page opens.